## @file
# PCI Library that layers on top of the PCI Root Bridge I/O Protocol.
#
# This library produces the APIs from the PCI Library and implements these APIs
#  by calling into the PCI Root Bridge I/O Protocol. The PCI Root Bridge I/O Protocol is
#  typically produced by a chipset specific DXE driver.
#  This library binds to the first PCI Root Bridge I/O Protocol in the platform. As a result,
#  it should only be used on platforms that contain a single PCI root bridge.
#
# Copyright (c) 2007 - 2018, Intel Corporation. All rights reserved.<BR>
#
#  This program and the accompanying materials
#  are licensed and made available under the terms and conditions of the BSD License
#  which accompanies this distribution. The full text of the license may be found at
#  http://opensource.org/licenses/bsd-license.php.
#  THE PROGRAM IS DISTRIBUTED UNDER THE BSD LICENSE ON AN "AS IS" BASIS,
#  WITHOUT WARRANTIES OR REPRESENTATIONS OF ANY KIND, EITHER EXPRESS OR IMPLIED.
#
#
##

[Defines]
  INF_VERSION                    = 0x00010005
  BASE_NAME                      = UefiPciLibPciRootBridgeIo
  MODULE_UNI_FILE                = UefiPciLibPciRootBridgeIo.uni
  FILE_GUID                      = 90EC42CB-B780-4eb8-8E99-C8E3E5F37530
  MODULE_TYPE                    = UEFI_DRIVER
  VERSION_STRING                 = 1.0
  LIBRARY_CLASS                  = PciLib|DXE_DRIVER DXE_RUNTIME_DRIVER DXE_SMM_DRIVER UEFI_DRIVER UEFI_APPLICATION

  CONSTRUCTOR                    = PciLibConstructor

#
# The following information is for reference only and not required by the build tools.
#
#  VALID_ARCHITECTURES           = IA32 X64 EBC
#

[Sources]
  PciLib.c


[Packages]
  MdePkg/MdePkg.dec


[LibraryClasses]
  BaseLib
  UefiBootServicesTableLib
  DebugLib

[Protocols]
  gEfiPciRootBridgeIoProtocolGuid               ## CONSUMES

[Depex.common.DXE_DRIVER, Depex.common.DXE_RUNTIME_DRIVER, Depex.common.DXE_SAL_DRIVER, Depex.common.DXE_SMM_DRIVER]
  gEfiPciRootBridgeIoProtocolGuid

